{"text_format":"1","workbook":"xls","n_sheets":1,"sheets":["Blad1 (2)"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Blad1 (2)","index":0,"n_rows":22,"n_cols":11,"rows_kept":22,"cut":false,"hidden":false,"merged":[[1,1,2,9],[4,8,4,10],[32,0,32,2],[32,11,32,12],[33,11,33,12],[24,11,24,12],[25,11,25,12],[26,11,26,12],[27,11,27,12],[28,11,28,12],[34,11,34,12],[35,11,35,12],[36,11,36,12],[29,11,29,12],[30,11,30,12],[31,11,31,12]],"flags":["formulas_cached_only"]}
[]
[null," Calculatie sheet benodigde deknadenrubber teakdek"]
[]
[]
["Hoe deze calculatie te gebruiken?",null,null,"Afmetingen in",null,"mm"]
[null,null,null,"breedte plank",null,42]
["Alleen de gele vakken invullen! ",null,null,"naad breedte",null,5]
["De rest wordt vanzelf ingevuld.",null,null,"naad diepte",null,8]
[]
[null,null,null,"Totaal m2",null,null,1]
[null,null,null,"aantal naden per m2:",null,null,21.27659574468085]
[null,null,null,"Totaal aantal meter naden:",null,null,21.27659574468085]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,"Aantal cartridges","Aantal worsten","Aantal tape"]
["Benodigde hoeveelheid",null,null,null,null,null,null,null,"305 ml ","592 ml  ","66m1 per rol"]
["TDS SIS440 deknadenrubber",null,null,null,null,1.021276595744681,"liter",null,4,2]
["Tape 3,5 & 5,5 mm","dikte tape afhankelijk van naadbreedte",null,null,null,21.27659574468085,"mtr",null,null,null,1.1]